Managing Your Work Environment > Setting Preferences > Audio Preferences >
ADAT Converter

The ADAT Converter area provides settings to configure the ADAT converter for audio I/O and monitoring. The ADAT Converter area and controls only appear if remote control of the ADAT converter is enabled in the software initialisation configuration file.

Lucid ADA 88192 Converter settings | Lucid ADA 8824 Converter settings

NoteDepending on the model of your ADAT converter, these controls may differ or provide slightly different functionality.

Input box
  Select either AES or Analog, depending on the Audio I/O device you are using.
Dig 1-2 box
  Select the type of I/O connection used for I/O channels 1 and 2: AES (XLR) or SPDIF (RCA).
A/D Sync box
  Select the sync source used by the ADAT converter for analog/digital conversion.
Meters box
  Select the signal that you want the LED meters on the ADAT to display.
Analog Inputs field
  Enter an analog input value.
Analog Outputs field
  Enter an analog output value.

NoteWith the Lucid 88192 ADAT converter, you have the choice of -10 dBV or +4 dBu as analog output values.

S.Clip box
  Enable to reset the peaking indication on the ADAT display. Peaks occur when the input signal is too hot for the ADAT converter.
Lock box
  Enable to prevent modifications of the ADAT converter from its front panel.
Reset button
  Resets ADAT converter parameters to their default values.