Editing > Audio > Using Input Strips >
Adjusting Pan Settings for an Input Strip

Once you assign the input strips to an output strip pair, you can use the pan faders to pan the input strip audio signal between the paired output strips.

To pan the signal between left and right output strips:

1. Click the pan fader for the pair of output signals that you want to pan and drag left or right to slide the pan fader.

   Drag: | To:
   --- | ---
   Left | Increase the amount of signal on the left (odd) output strip of the pair.
   Right | Increase the amount of signal on ther right (even) output strip of the pair.
   Centre | Send an equal amount of signal to the left and right output strips.

You can also specify numeric values in the pan fields to position the faders with precision.