Managing Projects and Media > Archiving >
Archiving and Restoring Mixed Resolution Projects
NoteFlare can create, write to, and read from file archives only.

Generally, archiving to data tape or filesystem is easier for archiving mixed-resolution projects, as clips of any resolution can be archived on the same medium. It is also possible to archive multiple-resolution projects to a VTR. This operation, however, may require multiple tapes with different timing corresponding to each segment resolution. Alternatively, you can use the Unlink tool to unlink media from clips of any resolution, archive unlinked clips, and then relink the media at restore time. See Unlinking Media from Clips in the Clip Library.

NoteBefore starting to archive a mixed-resolution project to a VTR, make sure you have enough tapes matching each resolution used in your project.

#### Topics in this section

- Archiving Clips Containing Sources with Different Bit Depths
- 8- and 10-bit VTR Archiving