Configuration Files > Software Initialisation File Keywords > ClipMgtDevice >
ClipMgtDevice Vtr

You can specify only one VTR for a VTR clip management device. The ClipMgtDevice Vtr keyword contains an optional start timecode parameter:

- If you specify a default start timecode for VTR archiving, the specified timecode is always used. You cannot override the default start timecode using the Archive menu.
- If you want to determine through the application the start timecode for archives created with a VTR, do not add the start timecode parameter.

The ClipMgtDevice Vtr keyword uses the following syntax

ClipMgtDevice Vtr[, <timecode>]

where <timecode> is an optional start timecode for the archive.

Example of use

ClipMgtDevice Vtr, 01:00:00:00