Configuration Files > Project Configuration File Keywords >
ColourSpace

The ColourSpace keyword defines how RGB/YUV conversions are handled. By default, for NTSC or PAL projects, the ITU-R BT.601-5 colour space is used. For DTV projects, the ITU-R BT.709-3 colour space is used.

The ColourSpace keyword uses the following syntax

ColourSpace <space_type>

where <space_type> is the colour space type used by the project.

Examples of use

Project | Keyword Example
--- | ---
NTSC and PAL standard projects (ITU-R BT.601-5) | ColourSpace 601
DTV standard projects (ITU-R BT.709-3) | ColourSpace 709
1920x1035 projects (SMPTE-240M) | ColourSpace 240