Inputting and Outputting Media > Clip Input/Output Using a VTR > Outputting Clips To a VTR >
HDCAM SR Stereo Tape Output

Using an HDCAM SR, you can ouput material to specially formatted stereoscopic tapes. Stereoscopic tapes essentially stores in an interlaced timing two progressive clips; a 60i (50i) “clip” contains two 30p(25p) clips.

To output sterescopic material to stereoscopic tape:

1. Ensure that the HDCAM SR is connected to the output card using a dual-link.
   ImportantIf you use the NVIDIA graphics card to output the stereoscopic material, the NVIDIA card downconverts the material to 8-bit.
2. Set the HDCAM SR VTR to the stereoscopic setting and insert a stereoscopic tape.
3. In the application, enter the Output Clip menu with a sterescopic clip. The presence of an S in the bottom right corner of a proxy indicates a sterescopic clip.
   NoteYou can output only clips at 23, 24, 50 or 59 fps, with a 1080i or 1080PsF resolution.
4. Output the clip. See Outputting a Single Clip.

   The Player in the Output Clip menu displays only the left-eye layer, but outputs both right- and left-eye layers, in a 4:2:2 colour space.