Conforming > Importing AAF Files > Preparing Sequences Cut in Avid for AAF Import >
Logging and Capturing from Tape in Avid

When capturing clips for offline edit sessions in Avid applications, you enter the tape name in the Tape Name field of the Capture Tool box. After importing the AAF in Flame, you recapture all the media from tape. It is this tape name, as entered in the Tape Name in Avid, that will indicate which tapes to use.

The following resolutions/framerates are supported for footage destined for Flame:

NTSC@23.976 PAL@25 720p60@59.94 1080p25@25 | NTSC@29.97 720p24@23.976 1080p24@23.976 1080i50@50 | PAL@24 720p60@29.97 1080p24@24 1080i60@59.94