Managing Your Work Environment > Setting Preferences >
LUT Preferences

Use the LUT preferences to import and list the 1D and 3D LUTs you can use in Flame. See General Workflow for LUTs.

You can use a hotkey to switch between the first ten LUTs in a 1D LUT list. Press Alt+Shift+1 for the first LUT, Alt+Shift+2 for the second LUT, and Alt+Shift+0 for the tenth LUT in the list.

You can use a hotkey to switch between the first ten LUTs in a 3D LUT list. Press Ctrl+Shift+1 for the first LUT, Ctrl+Shift+2 for the second LUT, and Ctrl+Shift+0 for the tenth LUT in the list.

(a) 3D LUT list

3D LUT List box
  Displays the list of 3D LUTs that you imported for use in Flame.
Import button
  Opens the Import LUT browser. Navigate to the 3D LUT file you want to use, and select it to load it to the 3D LUT list.
Delete button
  Deletes the selected LUT from the 3D LUT list.
Delete All button
  Deletes all LUTs from the 3D LUT list.

(a) LUT Type box(b) 3D LUT list

1D LUT List tab
  Displays the list of gamma LUTs that you defined and 1D LUTs that you imported for use in Flame.
LUT Type box
  Select whether you want to define a gamma LUT or import a 1D LUT file in the current row and assign the selected hotkey.
Import button
  Opens the Import LUT browser. Navigate to the file you want to use, and select it to load it to the 1D LUT list. This button is active when the LUT Type box is set to LUT file.
Value field
  Displays the gamma value. This field is active when the LUT Type box is set to Gamma.
Delete button
  Deletes the selected gamma or 1D LUTs from the list.
Delete All button
  Deletes all LUTs from the 1D LUT list.
Select button
  Apply the selected gamma or 1D LUT.

To define a gamma LUT:

1. Click the 1D LUT tab to display the 1D LUT list.
2. Select the row with the hotkey you want to assign to the gamma LUT.
3. Enter a gamma value in the Value field.

To apply a LUT from the 1D LUT list:

1. Click the 1D LUT tab.
2. Select the row with LUT you want to apply to the display.
3. Click Select.

   The filename of the applied LUT and its assigned hotkey display in blue.

   NoteWhen a ID or gamma LUT is applied it cannot be deleted, unless you click the Delete All button to clear the entire 1D LUT list.

To import a 1D or 3D LUT:

1. Click a tab to display the list for the type of LUT you want to import.
2. Select the row with the hotkey you want to assign to the LUT.
3. If the 1D LUT list is displayed, in the LUT file box, select LUT file.
4. Click the Import button.
5. In the file browser, navigate to the file you want to import.
6. Select the LUT file.

   The LUT file appears in the LUT list in the selected row.