Monitor Calibration > Applying Print LUTs for Viewing >

# Selecting Print LUTs

You can select up to three Print LUTs for quick comparison in a project. When your lab sends you the latest LUT, simply select it from the Calibrate menu. You can have any number of Print LUTs on the system.

To select Print LUTs for comparison:

1. (Optional) Import a LUT into the LUT list. See Importing a LUT File.
2. In the Calibrate menu, click 1.
3. Select a Print LUT from the Print LUT list.
   TipIf you copied or saved a LUT to the lut folder but the LUT is not listed, press CTRL+R to refresh the Print LUT list.

   The Print LUT is assigned to L1.

4. Repeat steps 1 and 2 to assign a Print LUT to L2 and L3.