Video Capture and Video Playout > Supported Video SDI and GFX SDI Rasters >

# Video SDI Rasters

The following table lists the video SDI rasters that are available for capture and playout in Lustre.

NoteThe Lustre HD Station does not support bit depths greater than 10-bit, input resolutions greater than 2K, or output resolutions greater than 1920x1080.

Video Type: | Pulldown: | Link Type: | Video Signal:
--- | --- | --- | ---
NTSC (29.97) | No | Single | 29.97 fps, 59.94 Hz, interlaced, 720x486, NDF timecode, YUV 4:2:2 data.
NTSC (29.97) | Yes | Single | 29.97 fps, 59.94 Hz, interlaced, 720x486, pulldown insert on playout and removal on capture, NDF timecode, YUV 4:2:2 data.
NTSC (29.97DF) | Yes | Single | 29.97 fps, 59.94 Hz, interlaced, 720x486, DF timecode, YUV 4:2:2 data.
NTSC (29.97DF) | No | Single | 29.97 fps, 59.94 Hz, interlaced, 720x486, pulldown insert on playout and removal on capture, DF timecode, YUV 4:2:2 data.
PAL (25) | No | Single | 25 fps, 50 Hz, interlaced, 720x576, YUV 4:2:2 data.
720p (50) | No | Single | 50 fps, progressive, 1280x720, YUV 4:2:2 data.
720p (50) | No | Dual | 50 fps, progressive, 1280x720, RGB 4:4:4 data.
720p (59.94) | No | Single | 59.94 fps, progressive, 1280x720, NDF timecode, YUV 4:2:2 data.
720p (59.94DF) | No | Single | 59.94 fps, progressive, 1280x720, DF timecode, YUV 4:2:2 data.
720p (59.94) | No | Dual | 59.94 fps, progressive, 1280x720, NDF timecode, RGB 4:4:4 data.
720p (59.94DF) | No | Dual | 59.94 fps, progressive, 1280x720, DF timecode, RGB 4:4:4 data.
720p (60) | No | Single | 60 fps, progressive, 1280x720, YUV 4:2:2 data.
720p (60) | No | Dual | 60 fps, progressive, 1280x720, RGB 4:4:4 data.
1080PsF (23.98) | No | Single | 23.98 fps, 72 Hz, segmented frames, 1920x1080, YUV 4:2:2 data.
1080PsF (23.98) | No | Dual | 23.98 fps, 72 Hz, segmented frames, 1920x1080, RGB 4:4:4 data.
1080p (23.98) | No | Single | 23.98 fps, progressive, 1920x1080, YUV 4:2:2 data
1080p (23.98) | No | Dual | 23.98 fps, progressive, 1920x1080, RGB 4:4:4 data
1080PsF (24) | No | Single | 24 fps, 48 Hz, segmented frames, 1920x1080, YUV 4:2:2 data.
1080PsF (24) | No | Dual | 24 fps, 48 Hz, segmented frames, 1920x1080, RGB 4:4:4 data.
1080p (25) | No | Single | 25 fps, progressive, 1920x1080, YUV 4:2:2 data
1080p (25) | No | Dual | 25 fps, progressive, 1920x1080, RGB 4:4:4 data
1080p (29.97) | No | Single | 29.97 fps, progressive, 1920x1080, NDF timecode, YUV 4:2:2 data
1080p (29.97) | No | Dual | 29.97 fps, progressive, 1920x1080, NDF timecode, RGB 4:4:4 data
1080p (29.97DF) | No | Single | 29.97 fps, progressive, 1920x1080, DF timecode, YUV 4:2:2 data
1080p (29.97DF) | No | Dual | 29.97 fps, progressive, 1920x1080, DF timecode, RGB 4:4:4 data
1080p (30) | No | Single | 30 fps, progressive, 1920x1080, NDF timecode, YUV 4:2:2 data
1080p (30) | No | Dual | 30 fps, progressive, 1920x1080, NDF timecode, RGB 4:4:4 data
1080i (25) | No | Single | 25 fps, 50 Hz, interlaced, 1920x1080, YUV 4:2:2 data.
1080i (25) | No | Dual | 25 fps, 50 Hz, interlaced, 1920x1080, RGB 4:4:4 data, RGB 4:4:4 data.
1080i (29.97) | No | Single | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, NDF timecode, YUV 4:2:2 data.
1080i (29.97) | No | Dual | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, NDF timecode, RGB 4:4:4 data.
1080i (29.97DF) | No | Single | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, DF timecode, YUV 4:2:2 data.
1080i (29.97DF) | No | Dual | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, DF timecode, RGB 4:4:4 data.
1080i (29.97) | Yes | Single | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, pulldown insert on playout and removal on capture, NDF timecode, YUV 4:2:2 data.
1080i (29.97) | Yes | Dual | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, pulldown insert on playout and removal on capture, NDF timecode, RGB 4:4:4 data.
1080i (29.97DF) | Yes | Single | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, pulldown insert on playout and removal on capture, DF timecode, YUV 4:2:2 data.
1080i (29.97DF) | Yes | Dual | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, pulldown insert on playout and removal on capture, DF timecode, RGB 4:4:4 data.
1080i (30) | No | Single | 30 fps, 60 Hz, interlaced, 1920x1080, NDF timecode, YUV 4:2:2 data.
1080i (30) | No | Dual | 30 fps, 60 Hz, interlaced, 1920x1080, NDF timecode, RGB 4:4:4 data.
1080i (30) | Yes | Single | 30 fps, 60 Hz, interlaced, 1920x1080, pulldown insert on playout and removal on capture, NDF timecode, YUV 4:2:2 data.
1080i (30) | Yes | Dual | 30 fps, 60 Hz, interlaced, 1920x1080, pulldown insert on playout and removal on capture, NDF timecode, RGB 4:4:4 data.
1556PsF (14/HSDL) | No | Single | 14 fps, segmented frame, 2048x1556, allows HSDL transfer, YUV 4:2:2 data.
1556PsF (15/HSDL) | No | Single | 15 fps, segmented frame, 2048x1556, allows HSDL transfer, YUV 4:2:2 data.
1556PsF (14/HSDL) | No | Dual | 14 fps, segmented frame, 2048x1556, allows HSDL transfer, RGB 4:4:4 data.
1556PsF (15/HSDL) | No | Dual | 15 fps, segmented frame, 2048x1556, allows HSDL transfer, RGB 4:4:4 data.