Working with Wiretap > Setting Up the Lustre Wiretap Project >

# Project Menu Settings

The following table explains the criteria to consider for each of the fields in the Project menu related to Wiretap projects.

Field | Criteria
--- | ---
Scans Full Home | To access a Stone FS or Standard FS, this field should have the same path as Project Home. To access 'published', unmanaged media (also called soft-imported media), populate this field with the path to the media residing on the shared network storage (for example, a SAN or NAS). For example, if the media is located in F:/SAN/Project/001, the Scans Full Home path should be F:/SAN.
Scans Half Home | To use proxies coming from a Stone FS or Standard FS, this field should have the same path as Project Home.
Renders Full Home | To render media to a Stone FS or Standard FS, browse to a clip library destination. This automatically sets the Wiretap render path. To render media to a shared network storage device (for example, a SAN or NAS), browse to a shared network destination. See Rendering Shots.
Renders Half Home | To render proxy media to a Stone FS or Standard FS, browse to a clip library destination. This automatically sets the Wiretap render path. To generate local proxies from media coming from a Stone FS or Standard FS, populate this field with the path to your local storage array. To generate local proxies from Published content, populate this field with the path to the local storage array or shared storage network.