Working with Wiretap > Before You Begin >

# Wiretap Gateway Limitations

When ingesting media using the Wiretap Gateway, please note the following:

- OpenEXR: Lustre supports ingest of OpenEXR in 16-bit float RGB format only. Files with other channels cannot be read in Lustre.
- RED Rocket Board: The RED Rocket board allows real-time decoding and debayering of RED media. For Lustre, it is supported in one configuration only. This is with Lustre installed on an HP Z800 workstation running Linux, and the Wiretap Gateway installed on a Mac OS workstation containing the RED Rocket board. The board must be installed in a PCI-E x16 slot. The network connection must be 10 GigE.