Video Capture and Video Playout > Supported Video SDI and GFX SDI Rasters >

# GFX SDI Rasters

The following table lists the GFX SDI rasters that are available for capture and playout in Lustre.

NoteThe Lustre HD Station does not support bit depths greater than 10-bit, input resolutions greater than 2K, or output resolutions greater than 1920x1080.

Video Type: | Pulldown: | Link Type: | Stereo: | Video Signal:
--- | --- | --- | --- | ---
NTSC (29.97) | No | Single | No | 29.97 fps, 59.94 Hz, interlaced, 720x486, NDF timecode, YUV 4:2:2 data.
NTSC (29.97) | Yes | Single | No | 29.97 fps, 59.94 Hz, interlaced, 720x486, pulldown insert on playout and removal on capture, NDF timecode, YUV 4:2:2 data.
PAL (25) | No | Single | No | 25 fps, 50 Hz, interlaced, 720x576, YUV 4:2:2 data.
720p (60) | No | Single | No | 60 fps, progressive, 1280x720, YUV 4:2:2 data.
720p (60) | No | Dual | No | 60 fps, progressive, 1280x720, RGB 4:4:4 data.
720p (59.94) | No | Single | No | 59.94 fps, progressive, 1280x720, NDF timecode, YUV 4:2:2 data.
720p (59.94) | No | Dual | No | 59.94 fps, progressive, 1280x720, NDF timecode, RGB 4:4:4 data.
1080PsF (23.98) | No | Single | No | 23.98 fps, 72 Hz, segmented frames, 1920x1080, YUV 4:2:2 data.
1080PsF (23.98) | No | Dual | No | 23.98 fps, 72 Hz, segmented frames, 1920x1080, RGB 4:4:4 data.
1080PsF (23.98) | No | Dual | Yes | 23.98 fps, 72 Hz, segmented frames, 1920x1080, RGB 4:4:4 data.
1080PsF (24) | No | Single | No | 24 fps, 48 Hz, segmented frames, 1920x1080, YUV 4:2:2 data.
1080PsF (24) | No | Dual | No | 24 fps, 48 Hz, segmented frames, 1920x1080, RGB 4:4:4 data.
1080PsF (24) | No | Dual | Yes | 24 fps, 48 Hz, segmented frames, 1920x1080, RGB 4:4:4 data.
1080PsF (25) | No | Dual | Yes | 25 fps, 48 Hz, segmented frames, 1920x1080, RGB 4:4:4 data.
1080PsF (30) | No | Dual | Yes | 30 fps, 48 Hz, segmented frames, 1920x1080, RGB 4:4:4 data.
1080p (23.98) | No | Dual | Yes | 23.98 fps, progressive, 1920x1080, NDF timecode, RGB 4:4:4 data.
1080p (24) | No | Single | No | 24 fps, progressive, 1920x1080, NDF timecode, YUV 4:2:2 data.
1080p (24) | No | Dual | No | 24 fps, progressive, 1920x1080, NDF timecode, RGB 4:4:4 data.
1080p (24) | No | Dual | Yes | 24 fps, progressive, 1920x1080, NDF timecode, RGB 4:4:4 data.
1080p (25) | No | Dual | Yes | 25 fps, progressive, 1920x1080, NDF timecode, RGB 4:4:4 data.
1080p (29.97) | No | Dual | Yes | 29.97 fps, progressive, 1920x1080, NDF timecode, RGB 4:4:4 data.
1080PsF (25) | No | Single | No | 25 fps, 50 Hz, segmented frames, 1920x1080, YUV 4:2:2 data.
1080PsF (25) | No | Dual | No | 25 fps, 50 Hz, segmented frames, 1920x1080, RGB 4:4:4 data.
1080i (25) | No | Single | No | 25 fps, 50 Hz, interlaced, 1920x1080, YUV 4:2:2 data.
1080i (25) | No | Dual | No | 25 fps, 50 Hz, interlaced, 1920x1080, RGB 4:4:4 data, RGB 4:4:4 data.
1080i (25) | No | Dual | Yes | 25 fps, 50 Hz, interlaced, 1920x1080, RGB 4:4:4 data, RGB 4:4:4 data.
1080p (29.97) | No | Single | No | 29.97 fps, progressive, 1920x1080, NDF timecode, YUV 4:2:2 data.
1080p (29.97) | No | Dual | No | 29.97 fps, progressive, 1920x1080, NDF timecode, YUV 4:2:2 data.
1080i (29.97) | No | Single | No | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, NDF timecode, YUV 4:2:2 data.
1080i (29.97) | No | Dual | No | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, NDF timecode, RGB 4:4:4 data.
1080i (29.97) | No | Dual | Yes | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, NDF timecode, RGB 4:4:4 data.
1080i (29.97) | Yes | Single | No | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, pulldown insert on playout and removal on capture, NDF timecode, YUV 4:2:2 data.
1080i (29.97) | Yes | Dual | No | 29.97 fps, 59.94 Hz, interlaced, 1920x1080, pulldown insert on playout and removal on capture, NDF timecode, RGB 4:4:4 data.
1080i (30) | No | Dual | Yes | 30 fps, 59.94 Hz, interlaced, 1920x1080, NDF timecode, RGB 4:4:4 data.
1080PsF (30) | No | Single | No | 29.97 fps, segmented frame, 1920x1080, NDF timecode, YUV 4:2:2 data.
1080PsF (30) | No | Dual | No | 29.97 fps, segmented frame, 1920x1080, NDF timecode, RGB 4:4:4 data.
1080PsF (30) | Yes | Single | No | 29.97 fps, 59.94 Hz, segmented frame, 1920x1080, pulldown insert on playout and removal on capture, YUV 4:2:2 data.
1080PsF (30) | Yes | Dual | No | 29.97 fps, 59.94 Hz, segmented frame, 1920x1080, pulldown insert on playout and removal on capture, RGB 4:4:4 data.
1080i (30) | No | Single | No | 30 fps, 60 Hz, interlaced, 1920x1080, NDF timecode, YUV 4:2:2 data.
1080i (30) | No | Dual | No | 30 fps, 60 Hz, interlaced, 1920x1080, NDF timecode, RGB 4:4:4 data.
1080i (30) | Yes | Single | No | 30 fps, 60 Hz, interlaced, 1920x1080, pulldown insert on playout and removal on capture, NDF timecode, YUV 4:2:2 data.
1080i (30) | Yes | Dual | No | 30 fps, 60 Hz, interlaced, 1920x1080, pulldown insert on playout and removal on capture, NDF timecode, RGB 4:4:4 data.
2Kp (23.98) | No | Single | No | 23.98 fps, 60 Hz, interlaced, 2048x1080, NDF timecode, YUV 4:2:2 data
2Kp (23.98) | No | Dual | No | 23.98 fps, 60 Hz, interlaced, 2048x1080, NDF timecode, RGB 4:4:4 data
2Kp (24) | No | Single | No | 24 fps, 60 Hz, progressive, 2048x1080, NDF timecode, YUV 4:2:2 data
2Kp (24) | No | Dual | No | 24 fps, 60 Hz, progressive, 2048x1080, NDF timecode, RGB 4:4:4 data
2Ki (25) | No | Single | No | 25 fps, 60 Hz, interlaced, 2048x1080, NDF timecode, YUV 4:2:2 data
2Ki (25) | No | Dual | No | 25 fps, 60 Hz, interlaced, 2048x1080, NDF timecode, RGB 4:4:4 data
2Kp (25) | No | Single | No | 25 fps, 60 Hz, progressive, 2048x1080, NDF timecode, YUV 4:2:2 data
2Kp (25) | No | Dual | No | 25 fps, 60 Hz, progressive, 2048x1080, NDF timecode, RGB 4:4:4 data
2Ki (29.97) | No | Single | No | 29.97 fps, 60 Hz, interlaced, 2048x1080, NDF timecode, YUV 4:2:2 data
2Ki (29.97) | No | Dual | No | 29.97 fps, 60 Hz, interlaced, 2048x1080, NDF timecode, RGB 4:4:4 data
2Kp (29.97) | No | Single | No | 29.97 fps, 60 Hz, progressive, 2048x1080, NDF timecode, YUV 4:2:2 data
2Kp (29.97) | No | Dual | No | 29.97 fps, 60 Hz, progressive, 2048x1080, NDF timecode, RGB 4:4:4 data
2Ki (30) | No | Single | No | 30 fps, 60 Hz, interlaced, 2048x1080, NDF timecode, YUV 4:2:2 data
2Ki (30) | No | Dual | No | 30 fps, 60 Hz, interlaced, 2048x1080, NDF timecode, RGB 4:4:4 data
2Kp (30) | No | Single | No | 30 fps, 60 Hz, progressive, 2048x1080, NDF timecode, YUV 4:2:2 data
2Kp (30) | No | Dual | No | 30 fps, 60 Hz, progressive, 2048x1080, NDF timecode, RGB 4:4:4 data