Browsing for Footage > Compressed Media Support > Browsing for Footage with the Wiretap Gateway > Wiretap Gateway Supported Ingest File Formats >

# Overview

This appendix lists the image and audio file formats supported by the Wiretap Gateway server, for ingest. Use the tables in this appendix to determine if a particular digital image sequence or container format can be recognized by the Wiretap Gateway.

An image sequence is a series of sequentially numbered files, traditionally the result of scanning film stock at high resolution to produce a digital intermediate. Here, each file contains the digital scan of an individual frame. Common image sequence formats include Cineon®, DPX and Tiff. The type of image sequence file on hand is usually revealed by its extension.

In contrast, container formats, also called “wrapper” formats, can contain image sequences (commonly called streams or essences) and audio, compressed using a variety of compression algorithms (codecs) into a single file. Container formats do not impose specific video or audio codecs upon the media they contain. Rather, a container format defines only how the video, audio and other data is stored within the container itself. Unlike image sequences, it is not possible to tell by looking at the extension what kind of video or audio is inside a container format.