Browsing for Footage > Compressed Media Support > Browsing for Footage with the Wiretap Gateway > Wiretap Gateway Supported Ingest File Formats > Supported Image Container Formats >

# Supported DNxHD MXF File Codecs

The Wiretap Gateway supports the import of MXF files encoded with Avid® DNxHD® codec.

NoteMaterial at 1080i encoded with the DNxHD 145 codec sometimes uses a thin raster frame format, denoted as 145-TR. It uses an frame size of 1440x1080 (NTSC) or 1280x1080 (PAL). Enable Scale to Full HD to scale the material to the full 1920x1080 frames. Disable Scale to Full HD to use the thin raster frame.

Resolution | Frame Rate | Avid DNxHD CODEC | Bit Depth
--- | --- | --- | ---
1080i | 59.94 | DNxHD 220x | 10
DNxHD 220 | 8
DNxHD 145 | 8
50 | DNxHD 185x | 10
DNxHD 185 | 8
DNxHD 120 | 8
1080p | 29.97 | DNxHD 220x | 10
DNxHD 220 | 8
DNxHD 145 | 8
DNxHD 45 | 8
25 | DNxHD 185x | 10
DNxHD 185 | 8
DNxHD 120 | 8
DNxHD 36 | 8
23.976 & 24 | DNxHD 175x | 10
DNxHD 175 | 8
DNxHD 115 | 8
DNxHD 36 | 8
720p | 59.94 | DNxHD 220x | 10
DNxHD 220 | 8
DNxHD 145 | 8
50 | DNxHD 175x | 10
DNxHD 175 | 8
DNxHD 115 | 8
29.97 | DNxHD 110x | 10
DNxHD 110 | 8
DNxHD 75 | 8
23.976 & 25 | DNxHD 90x | 10
DNxHD 90 | 8
DNxHD 60 | 8