Monitor Calibration >

# Applying Print LUTs for Viewing

Use Print LUTs, obtained from your film lab, to apply preset gamma correction. Print LUTs are specially designed by your lab to ensure an accurate display of your film stock images by simulating a film print look. Print LUTs may be updated several times a day to ensure proper calibration with the lab. Save the Print LUTs in the C:\Program Files\Autodesk\Lustre 2010\lut folder if running the Windows version of Lustre, or in the /usr/Autodesk/lustre_2010/lut directory if running the Linux version of Lustre.

NoteIn Lustre, LUTs used to calibrate the monitor are applied from the 16-bit result buffer and have a higher quality than those produced on the graphics card.

#### Topics in this section

- Selecting Print LUTs
- Switching between Print LUTs