Working with Wiretap >

# Dust Bust and Marry Grade

It is possible to perform dust removal on media imported via Wiretap. However, since media stored on a Stone FS or Standard FS filesystem cannot be replaced by Lustre, you can create dust metadata for use when rendering media only.

NoteThe render options within the Image>Dust menu are inactive when media is imported from the Wiretap server or Wiretap Gateway. You can only render by using the Dust option within the Render>Local menu.

Media imported by Wiretap can also be used to generate Marry Grade data. However, since it is not possible to write Marry Grade files to Stone FS or Standard FS filesystems, the Marry Grade files are stored in the project’s Full or Half Scan location. In the Marry Grade folder, a WT (Wiretap) folder is automatically created. Within it, a hierarchy of folders contain the Marry Grade data.