Browsing for Footage > Compressed Media Support > Browsing for Footage with the Wiretap Gateway > Wiretap Gateway Supported Ingest File Formats > Supported Image Container Formats >

# Support for AVC-HD Files

It is now possible to import AVC-HD content in Lustre through the Wiretap Gateway. Video and audio media, and timecode tracks are supported.

NoteOnly PCM audio is supported. Some cameras can record AC-3 audio, but this format is not supported. Only the video portion of AVC-HD media with AC-3 audio content is accessible from the application.