Browsing for Footage > Compressed Media Support > Browsing for Footage with the Wiretap Gateway > Wiretap Gateway Supported Ingest File Formats >

# Supported Image Sequence Formats

The Wiretap Gateway server supports ingest of the following image sequence file formats.

File Format | Bit Depth | Default Extension
--- | --- | ---
Alias® | 8-bit | als
Cineon® | 10-bit | cin
DPX | 8-bit, 10-bit, and 12-bit | dpx
Jpeg | 8-bit | jpg
Macintosh® Pict | 8-bit | pict
OpenEXR | 16-bit int, 16-bit float, 32-bit float | exr
Pixar | 8-bit | picio
SGI® | 8-bit and 16-bit | sgi
Softimage® | 8-bit | pic
TARGA® | 8-bit | tga
Tdi/Maya® | 8-bit and 16-bit | iff
Tiff | 8-bit and 16-bit | tif
Wavefront® | 8-bit and 16-bit | rla

NoteThe Wiretap Gateway supports ingest of OpenEXR 16-bit RGB float only. Files with other channels, RGBA, for example, cannot be read in Lustre.