Video Capture and Video Playout >

# Supported Video SDI and GFX SDI Rasters

When capturing from or recording to a VTR, you must select the appropriate raster. The raster defines the video capture/playout SDI timing and the graphic SDI timing. Lustre supports many DVS and AJA video SDI rasters and GFX SDI graphics rasters. See Video SDI Rasters and GFX SDI Rasters.

In past releases of Lustre, you had to define a colour conversion matrix in a configuration file. Starting with Lustre 2012, you no longer need to do this. The correct conversion matrix is automatically configured when you select a video SDI raster. The matrix name will be displayed in the VTR status box located in the Editing > Capture and Editing > Playout menus.

NoteYou cannot enable both a GFX and a Video raster, except when working with audio, when you can use a DVS/AJA raster for audio, and a GFX for graphics.

#### Topics in this section

- Video SDI Rasters
- GFX SDI Rasters