Managing Projects and Media > Archiving > Creating a VTR Archive >
HD Board 1080 Line Video Timings

If you are working with an HD board and you selected the 1920x1080 video timing option in the Video Timing box when you started your project, you should specify the exact 1080 line video timing (including framerate) that you are using in the 1080 Video Timing box in the Engineering menu. See Setting Video Input and Output Engineering Menu Controls.

NoteIf you selected “No VTR Selected” in the Video Timing box, you must specify the video timing using the 1080 Video Timing box.