Conforming > Exporting EDLs > About the Export EDL Menu >
Output Options Group

Before outputting an EDL, select the material that is output, the length of handles (if any), the method of exporting timewarps, the output tape ID, and the starting timecode.

(a) Output Type box(b) Limit Handles field(c) Timewarp Mode box(d) Output Tape field(e) Start Timecode field(f) Frame Code Mode box

Output Type box
  Select the material to output to a VTR.

Select: | To:
--- | ---
Output All Material | Output all source clips and clips created in Flame.
Output Generated Only | Output only clips created in Flame.
No Output | Not output any clips. Only the EDL is generated.

Limit Handles button
  Enable to export the source clip with a specified maximum number of frames before and after.
Limit Handles field
  Enter a value for the number of frames used before and after the edit.
Timewarp Mode box
  Select how timewarps are output.

Select: | To:
--- | ---
EDL Varispeed | Create a timewarp command in the EDL that plays the clip at the timewarp speed.
Rendered Source | Render the timewarp before outputting the clip to the VTR. This creates a newly rendered clip and replaces the timewarp.

NoteThere is no standard EDL format that recognizes timewarps created using the Timewarp Editor. If you create a timewarp using a custom curve, you must use the Rendered Source option; otherwise, the timewarp curve is lost.

Output EDL Material button
  Output the EDL material to a VTR. The EDL Output module appears, which is comprised of the same controls as the Clip Output module.
Save Output to Library button
  Output the EDL material as a clip in the clip library. The EDL is output to the same library reel from which you originally accessed the Export EDL menu.
Output Tape field
  Enter a tape ID for the output material. The Output tape ID is used in the EDL to reference the destination of the material. Note that the edit's original tape ID is added to the Comment field. This is useful if you want to trace an element to its original source.
Start Timecode field
  Enter a value to specify the start timecode for the output material. If the start timecode is 01:00:00:00, the clip with all the material begins at 01:00:00:00. The start timecode is used in the EDL to reference the location of material.
Frame Code Mode box
  Select the drop frame mode for the output material. Select DF (drop frame) or NDF (non-drop frame) format.