Inputting and Outputting Media > Importing Media Files and Sequences > Media Files Import Preferences and Import History Options > RED-Only Preferences >
Debayering Menu

Debayering
  Select the level of quality required from the debayering algorithm. Higher resolutions are significantly more processing intensive.
  NoteThe debayering setting is the most resource-intensive setting. Try using the level of debayering the most appropriate for your work.
Detail
  Select the level of detail extraction required.
OLPF Compensation
  Select the level of Optical Low Pass Filter (OLPF) compensation to use. OLPF is a type of sharpening used to compensate for the optical anti-aliasing filter, which can induce softening of the image during recording.
Denoise
  Select the level of noise reduction applied to the debayered clip.