Managing Your Work Environment > Setting Preferences > Broadcast Monitor Preferences >
Broadcast Stereo

Use the Broadcast Stereo preferences to set how the broadcast monitor displays stereoscopic images.

NoteBroadcast Stereo options depend on your hardware configuration. As well, the option displayed is the same as the one selected in the Player. If you change the option in one location, it is changed automatically in the other location.

Broadcast Stereo box
  Select the stereoscopic display option that best works for you. This option determines how the Player and the broadcast monitor viewport display stereoscopic material.

Select: | If you use:
--- | ---
Anaglyph | A standard broadcast monitor. (Default option)
Interlaced | A broadcast monitor capable of displaying a stereoscopic image as an interlaced image where one field is the left-eye and the other is the right eye.
Dual Output | A broadcast monitor solution which requires a dual-SDI output, such as a dual-projector setup.

NoteIf there is no broadcast monitor connected or if the Broadcast Monitor box is set to Off, the Broadcast Stereo box is set to Stereo Anaglyph.

Stereo Option box
  If the Broadcast Stereo box is set to Interlaced, select the field to use as the left eye. If the Broadcast Stereo box is set to Anaglyph, select the type of anaglyph setting to use.

Select: | To view:
--- | ---
Diff | The difference between the two images, with the minimum and maximum threshold values non clamped.
Diff Clamped | The difference between the two images, with the minimum and maximum threshold values clamped.
Blend | A combined image of the two tracks.
Mono | The image with just the anaglyph effect. The RGB values are removed from the display.
Dubois | The image with reduced ghosting between the left and right eyes.