Configuration Files > About Project Configuration Files > Project Configuration File Templates >
Supported HD Formats in Project Templates

The names of project templates for HD formats contain a string that identifies the format's resolution, framerate, and scan mode.

Project configuration templates with the following string in their name: | Correspond to the following HD format:
--- | ---
1280x720@5994p | 1280x720 progressive scan at 59.94 frames per second (720/59.94p, SMPTE-296M)
1280x720@5000p | 1280x720 progressive scan at 50 frames per second (720/50p, SMPTE-296M)
1280x720@6000p | 1280x720 progressive scan at 60 frames per second (720/60p, SMPTE-296M)
1920x1080@23976psf | 1920x1080 progressive segmented frame at 23.976 frames per second (1080/23976psf, SMPTE-274M, RP-211)
1920x1080@24000psf | 1920x1080 progressive segmented frames at 24 frames per second (1080/24psf, SMPTE-274M, RP-211)
1920x1080@25000psf | 1920x1080 progressive segmented frames at 25 frames per second (1080/25psf, SMPTE-274M, RP-211)
1920x1080@50i | 1920x1080 interlaced scan at 50 fields per second (1080/50i, SMPTE-274M)
1920x1080@5994i | 1920x1080 interlaced scan at 59.94 fields per second (1080/59.94i, SMPTE-274M)
1920x1080@6000i | 1920x1080 interlaced scan at 60 fields per second (1080/60i, SMPTE-274M)