Editing > Audio > About Auxiliary Effects >
Delay

The Delay effect temporarily stores an audio signal then plays it back after a period of time (Delay). The delayed signal may fed back into the recording again (Feedback), to create the sound of a repeating, decaying echo. It is different from reverb, which creates a “reflected” sound using a different technique. The Delay effect is based on a simple algorithm made of two independent mono delay lines.

Control | Values | Description
--- | --- | ---
Delay | 0 - 20000 ms | Defines the amount of time to delay the signal. Default is 250 ms.
Feedback | 0% - 100% | Defines the number of times to repeat the signal. Default is 15%.
Gain | -96 - 0 dB | Default is -12 dB.