Configuration Files > Software Initialisation File Keywords >
Video

The Video keyword initialises the video device and specifies the video input type.

Video device
  The video input devices supported are AJA_KONA3G and AJA_OEM2K.
Default video input format
  The default video input format that corresponds to the input configuration of the video card. This setting is overridden by the video input formats specified by the lines you uncomment for each VTR under the Vtr keyword heading.
The Video keyword uses the following syntax

Video <video_device>, <default_video_format>

Where: | Is:
--- | ---
<video_device> | The video card used by your workstation. It can take the following values: AJA_KONA3G AJA_OEM2K
<default_video_format> | The video input type. For all AJA cards, the supported video input types are Serial1 and SerialDual.

Examples of use

Video AJA_KONA3G, Serial1