Monitor Calibration >

# Calibrating for Dual-Head Mode

If the video card on the Lustre system is set to Dual-Head mode, you can set different LUTs for each monitor. This is useful when using different display types, such as a monitor and a plasma screen.

To set different LUTs:

1. (Optional) Import a LUT into the LUT list. See Importing a LUT File.
2. In the Calibrate menu, click 1 for the main monitor and select a 3D LUT for the main LUT.
   NoteA 3D LUT is processed directly on the video card and therefore ensures better performance in Lustre.
3. Click 2 and select any LUT for the second monitor.
   NoteThis setup will not affect playback speed unless a 3D LUT is also chosen for the second monitor. In this case, the playback rate will be approximately 18 fps.