Browsing for Footage > Compressed Media Support > Browsing for Footage with the Wiretap Gateway > Wiretap Gateway Supported Ingest File Formats > Supported Image Container Formats >

# Support for GoPro HD MP4 Files

GoPro camera records H.264 files with an "mp4" extension. Files from this camera are supported by Wiretap Gateway Server.

The following frame rates and resolution are now supported (with audio):

- 1920x1080 (16x9, 29.97p and 25p)
- 1280 x 960 (4x3, 29.97, 25p)
- 1280 x 720 (16x9, 25p, 29.97p & 59.94p)
- 848x480 (16x9, 25p, 29.97p & 59.94p)

Due to limitation in the GoPro 59.94p files, the application assigns to those files the timing of the project. So if your project is set at 30fps, 59.94 GoPro files are imported at 30fps. To play back 59.94 GoPro files correctly, you must be using a 59.94 project.