Video Capture and Video Playout > Capturing Material >

# Removing Pulldown when Capturing

Depending on the type of source material you are working from, you may need to remove 3:2 pulldown frames at capture time. For more information about 3:2 pulldown, see About 3:2 Pulldown.

NoteInconstant cadence material (i.e., re-edited material) may produce jittery results.

To remove 3:2 pulldown during capture:

1. Click Pulldown.
2. Use the VTR to shuttle to the first frame you want to capture.

   (a) Pulldown Field buttons

3. Enable the Pulldown Field button that matches the field composition of that frame.