The Tangent CP100 Control Surface > Secondary Colour Grading >

# Applying Secondaries to the Shot

Use the second row of buttons on the left side of the control surface to set basic parameters for secondaries.

Press: | To:
--- | ---
Sec | Switch on and off the current secondary.
Keyer | Switch on and off the Keyer for the current secondary.
Invert | Invert the key for the current secondary.
Reset | Reset the key for the current secondary.

Enable the Sec button to apply the displayed secondary to the shot.