Autodesk Developer Network 2011
Autodesk
Small Enhancements and Changes
§Spare and space circuits
§A new ElectricalSystem.CircuitType property identifies the type of an electrical circuit (circuit, spare or space), and the ElectricalSystem.AddToCircuit method throws an exception when the system is a spare or space circuit
§Cable tray and conduit domain
§The Autodesk.Revit.DB.Domain enumeration adds a new value to represent cable tray and conduit
§Connector
§New read-only properties added for JointType, GenderType and EngagementLength
§MEPSystem
§New property MEPSystem.IsEmpty
§Graphical warnings for disconnects
§New ‘show graphical warning’ properties and setters on the Application class
§Space properties
§New property Space.BaseHeatLoadOn indicates if the value of Space.LatentHeatGainperPerson and Space.SensibleHeatGainperPerson properties has the default value or is user defined
§Fitting methods
§Document methods to create new fittings no longer remove unused or dangling curve connectors